{"text_format":"2","workbook":"xls","n_sheets":2,"sheets":["일반열람대","일반열람대2"],"not_rendered":{"charts":0,"images":7,"macros":0,"external_links":1,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"일반열람대","index":0,"n_rows":64,"n_cols":14,"rows_kept":64,"cut":false,"hidden":false,"merged":[[31,0,48,0],[50,0,61,0]],"flags":["formulas_cached_only"]}
[]
["일반열람대",{"$nulls":12},"School Study Desk"]
{"$rows_empty":27}
[" 780X670X1670  (WXDXH)"]
[]
["제품특징\n\n(기  능)"]
[]
[]
[null," ·","엔드리스 방식의 열람공간 확대 시스템"]
[null,null,"(연결형의 측판이 독립형과 연결형의 중측판이 되고 독립형 측판이 최종 마감 측판이 됨)"]
[]
[null," ·","상판 / 측판 / 수평 덕트의 배선 처리"]
[]
[null," ·","시건 기능이 있는 개인 수납 공간"]
[]
[null," ·","도어에 최고급 Concealed 힌지 부착"]
[]
[null," ·","하부 수납 / 발받침 기능의 밑선반"]
[]
[null," ·","측판 하부에 높낮이조절기능이 있는 글라이더 부착"]
[]
[]
[]
[]
["제품특징\n\n(디자인)"]
[]
[]
[null," ·","손잡이를 삭제한 도어는 깨끗한 외관과 사용상의 편리함을 제공"]
[]
[null," ·","라운드 디자인의 측판은 기존 공부방 가구와 차별화"]
[]
[null," ·","상판 및 측판(BE/CM)과 도어(IV)에 TWO-TONE 칼라를 적용하여 기존의 딱딱한 이미지에서 탈피하고"]
[]
[null,null,"이용자에게 따뜻하고 안정적이며 고급스러운 느낌 부여"]
[]
[]
[]
["※ 본 시방서의 내용은 계속되는 제품의 연구, 개발로 인해 일부 변경될 수 있습니다."]

{"sheet":"일반열람대2","index":1,"n_rows":62,"n_cols":14,"rows_kept":62,"cut":false,"hidden":false,"merged":[[31,1,40,1],[42,1,59,1]],"flags":["formulas_cached_only"]}
[]
[null,"일반열람대",{"$nulls":11},"School Study Desk"]
{"$rows_empty":27}
[null,"780X670X1670  (WXDXH)",{"$nulls":5},"758X670X1670  (WXDXH)"]
[]
[null,"자    재"]
[]
[null,null," ·","측판",":","22T 파티클보드(PB) ＋ 양면 LPM + 4면 2.0T ABS엣지"]
[null,null," ·","상판",":","22T 파티클보드(PB) ＋ 양면 LPM + 1면 2.0T ABS엣지"]
[null,null," ·","윗선반/밑선반/밑판",":","18T 파티클보드(PB) ＋ 양면 LPM + 1면 1.0T ABS엣지"]
[null,null," ·","뒷판",":","18T 파티클보드(PB) ＋ 양면 LPM + 2면 1.0T ABS엣지"]
[null,null," ·","도어",":","18T 파티클보드(PB) ＋ 양면 LPM + 4면 1.0T ABS엣지"]
[null,null," ·","수평덕트",":","CR 1.2T"]
[]
[]
[]
[null,"제작공정"]
[]
[null,null," ·","측판/도어",":","    재단 → PB 재단"]
[{"$nulls":5},"    엣지접착 → 4면 PB 단면에 엣지 접착"]
[{"$nulls":5},"    세공 → 조립용 홀 가공"]
[]
[null,null," ·","상판/윗선반/밑선반/밑판",":","    재단 → PB 재단"]
[{"$nulls":5},"    엣지접착 → 1면 PB 단면에 엣지 접착"]
[{"$nulls":5},"    세공 → 조립용 홀 가공"]
[]
[null,null," ·","뒷판",":","    재단 → PB 재단"]
[{"$nulls":5},"    엣지접착 → 2면 PB 단면에 엣지 접착"]
[{"$nulls":5},"    세공 → 조립용 홀 가공"]
[]
[null,null," ·","수평덕트",":","    절곡"]
[{"$nulls":5},"    도장 → 정전 분체도장"]
[]
[]
[]
[null,"※ 본 시방서의 내용은 계속되는 제품의 연구, 개발로 인해 일부 변경될 수 있습니다."]