{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":15,"n_cols":4,"rows_kept":15,"cut":false,"hidden":false,"merged":[[1,0,12,0],[13,0,13,1],[14,0,14,1],[0,0,0,1]]}
["항목",null,"Spec.","비고"]
["VNA","Frequency range","10 MHz to 67 GHz"]
[null,"Number of ports",4]
[null,"Dynamic range"]
[null,"50 MHz to 50 GHz","120 dB"]
[null,"50 GHz to 67 GHz","110 dB"]
[null,"Directivity","40 dB"]
[null,"Source match","40 dB"]
[null,"Load match","40 dB"]
[null,"Power"]
[null,"Max output @ 67 GHz","5 dBm"]
[null,"Power accuracy @ 67 GHz","3 dB"]
[null,"Power linearity @ 67 GHz","1 dB"]
["Cable",null,"50 ohm, 1.85 mm, ~24 inch","4개"]
["Calibration kit",null,"1.85 mm, m/f each"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}