{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["사물함"],"not_rendered":{"charts":0,"images":2,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"사물함","index":0,"n_rows":61,"n_cols":4,"rows_kept":61,"cut":false,"hidden":false,"merged":[[22,1,22,14],[28,1,44,1],[46,1,58,1]],"flags":["formulas_cached_only"]}
{"$rows_empty":24}
[null,"409X430X1198  (WXDXH)  - 2인용 사물함 (2단1열)"]
[null,"805X430X1198  (WXDXH)  - 4인용 사물함 (2단2열)"]
[null,"1200X430X1198  (WXDXH)  - 6인용 사물함 (2단3열)"]
[]
[null,"제품특징\n\n(기   능)"]
[]
[]
[null,null,"  ·","학생들이 자물쇠를 이용하여 손쉽게 도어를 시건할 수 있는 구조로 설계하였음"]
[]
[null,null,"  ·","시건장치 겸용 손잡이는 P.C(폴리카보네이트)로 제작하여 내구성이 우수함"]
[]
[null,null,"  ·","사용자의 안전성을 고려한 매립형 손잡이"]
[]
[null,null,"  ·","도어마다 네임플레이트를 부착하여 학생들이 간편하게 이름표를 부착할 수 있음"]
[]
[null,null,"  ·","270도 힌지를 적용하여 도어의 완전 열림이 가능함"]
[]
[null,null,"  ·","하부에 높이조절 글라이드를 부착하여 편리하게 수평을 조절할 수 있으며, 습기로 인한 제품 손상 방지"]
[]
[]
[]
[]
[null,"제품특징\n\n(디자인)"]
[]
[]
[null,null,"  ·","형태의 견고함과 심플함을 살리기 위하여 블랙 엣지를 적용"]
[]
[null,null,"  ·","손잡이 부분이 도드라지지 않고 전체적인 부속으로 작용할 수 있도록 심플하게 디자인"]
[]
[null,null,"  ·","디테일이 전체를 파괴하지 않도록 네임플레이트와 시건장치를 일체화하여 심플함을 강조"]
[]
[null,null,"  ·","도어와 바디의 투톤컬러 조합으로 세련된 디자인을 추구"]
[]
[]
[]
[]
[null,"※ 본 시방서의 내용은 계속되는 제품의 연구, 개발로 인해 일부 변경될 수 있습니다."]