{"text_format":"2","workbook":"xls","n_sheets":2,"sheets":["제품 특징 (2)","의자"],"not_rendered":{"charts":0,"images":2,"macros":0,"external_links":1,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"제품 특징 (2)","index":0,"n_rows":59,"n_cols":18,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
["  UCH9 series             ",{"$nulls":13},"CONFERENCE CHAIR"]
{"$rows_empty":25}
["   UCH0009 : 490 × 505 × 790 (W × D × H)"]
[]
[]
[]
[]
[null,"  · 내구성이 강한 고품질의 P.P (폴리프로필렌)로 만들어진 등좌판"]
[]
[null,"  · Ø12 환봉으로 일체화된 프레임을 제작하고 고품질 분체도장 마감"]
["제품특징"]
[null,"  · 다리프레임 하부에 나일론 소재의 글라이드를 부착하여 소음 방지"]
["(기 능)"]
[null,"  · 사용하지 않을 때는 의자를 적층할 수 있어 공간 효율성을 높일 수 있음",{"$nulls":15},"  "]
[]
[]
[]
[]
[null," ",null,"       "]
[]
[]
[]
[null,"  · 복합소재의 효율적인 사용을 통해 디자인과 내구성을 겸비"]
[]
[null,"  · 다양한 공간에 사용할 수 있는 간결한 디자인"]
["제품특징"]
[null,"  · Red, Blue, Dark Grey 3가지 색상의 등좌판과 Metalic Silver 계통의 프레임의 색상 조화"]
["(디자인)"]
[{"$nulls":17},"  "]
[]
[]
[]
[]
[null," ",null,"       "]

{"sheet":"의자","index":1,"n_rows":53,"n_cols":14,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
["  UCH9 series             ",{"$nulls":12},"CONFERENCE CHAIR"]
{"$rows_empty":25}
["   UCH0009 : 490 × 505 × 790 (W × D × H)"]
[]
[]
[]
[]
[null," ·","등   좌   판",":","P.P (폴리프로필렌)"]
[]
[null," ·","프   레   임",":","Ø12 환봉"]
[]
[null," ·","글 라 이 드",":","PA6 (나일론)"]
["자    재"]
{"$rows_empty":8}
[null," ·","등   좌   판",":","사출 성형"]
[]
[null," ·","프   레   임",":","Ø12 환봉 Cutting → 벤딩 (CNC 벤딩기) → 브라켓 용접 → 분체도장"]
[]
["제작공정"," ·","글 라 이 드",":","사출 성형"]
[]
[null," ·","전 체 조 립",":","전체 조립 → 기능 확인 → 포장"]