{"text_format":"2","workbook":"xlsx","n_sheets":2,"sheets":["기기","시공비"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"기기","index":0,"n_rows":174,"n_cols":4,"rows_kept":174,"cut":false,"hidden":false,"merged":[[31,1,35,1],[4,1,6,1],[4,2,6,2],[7,1,9,1],[7,2,9,2],[10,1,12,1],[13,1,15,1],[16,1,18,1],[19,1,21,1],[22,1,24,1],[25,1,27,1],[28,1,30,1],[91,1,93,1],[36,1,40,1],[41,1,45,1],[46,1,50,1],[51,1,55,1],[56,1,60,1],[61,1,65,1],[66,1,70,1],[71,1,75,1],[76,1,80,1],[81,1,85,1],[86,1,90,1],[94,1,96,1],[97,1,99,1],[100,1,102,1],[103,1,105,1],[106,1,108,1],[124,1,128,1],[129,1,133,1],[134,1,138,1],[109,1,113,1],[114,1,118,1],[119,1,123,1],[149,1,153,1],[149,2,153,2],[154,1,158,1],[154,2,158,2],[139,1,143,1],[144,1,148,1],[144,2,148,2],[159,1,163,1],[159,2,163,2],[164,1,168,1],[164,2,168,2],[169,1,173,1],[169,2,173,2]]}
[]
[null,null,"<기기 사양서> - 시공비 사양은 별도 탭 참조"]
[]
[null,"순번","기기명","사양표"]
[null,1,"벽걸이 인버터 11평형 ","■전원:220/60V"]
[null,null,null,"■냉방소비전력:　1.04kw"]
[null,null,null,"■냉방능력:　4.2kw"]
[null,2,"벽걸이 인버터 13평형 ","■전원:220/60V"]
[null,null,null,"■냉방소비전력:　1.48kw"]
[null,null,null,"■냉방능력:　5.2kw"]
[null,3,"냉방전용 인버터","■전원:220/60V"]
[null,null,"16평형 ","■냉방소비전력:　1.9kw"]
[null,null,null,"■냉방능력:　6.5kw"]
[null,4,"냉방전용 인버터","■전원:220/60V"]
[null,null,"18평형 ","■냉방소비전력:　2.3kw"]
[null,null,null,"■냉방능력:　7.2kw"]
[null,5,"냉방전용 PAC","■전원:220/60V"]
[null,null,"23평형 ","■냉방소비전력:　2.5kw"]
[null,null,null,"■냉방능력:　8.3kw"]
[null,6,"냉방전용 인버터","■전원:220/60V"]
[null,null,"30평형 ","■냉방소비전력:　3.2kw"]
[null,null,null,"■냉방능력:　10.0kw"]
[null,7,"냉방전용 인버터","■전원:220/60V"]
[null,null,"40평형 ","■냉방소비전력:　4.4kw"]
[null,null,null,"■냉방능력:　14.5kw"]
[null,8,"냉방전용 PAC","■전원:380/60V"]
[null,null,"58평형 ","■냉방소비전력:　7.55kw"]
[null,null,null,"■냉방능력:　21.0kw"]
[null,9,"냉방전용 PAC","■전원:380/60V"]
[null,null,"83평형 ","■냉방소비전력:　12.5kw"]
[null,null,null,"■냉방능력:　30.0kw"]
[null,10,"냉난방 인버터","■전원:220/60V"]
[null,null,"15평형 ","■냉방소비전력:　1.8kw"]
[null,null,null,"■난방소비전력:　2.2kw"]
[null,null,null,"■냉방능력:　6.0kw"]
[null,null,null,"■난방능력:　7.2kw"]
[null,11,"냉난방 인버터","■전원:220/60V"]
[null,null,"18평형 ","■냉방소비전력:　2.0kw"]
[null,null,null,"■난방소비전력:　2.3kw"]
[null,null,null,"■냉방능력:　7.2kw"]
[null,null,null,"■난방능력:　8.5kw"]
[null,12,"냉난방 인버터","■전원:220/60V"]
[null,null,"23평형 ","■냉방소비전력:　2.85kw"]
[null,null,null,"■난방소비전력:　3.00kw"]
[null,null,null,"■냉방능력:　8.3kw"]
[null,null,null,"■난방능력:　9.2kw"]
[null,13,"냉난방 인버터","■전원:220/60V"]
[null,null,"30평형","■냉방소비전력:　3.4kw"]
[null,null,null,"■난방소비전력:　3.7kw"]
[null,null,null,"■냉방능력:　11.0kw"]
[null,null,null,"■난방능력:　13.2kw"]
[null,14,"천정형냉난방","■전원:220/60V"]
[null,null,"10평형 ","■냉방소비전력:　1.43kw"]
[null,null,null,"■난방소비전력:　1.78kw"]
[null,null,null,"■냉방능력:　4.0kw"]
[null,null,null,"■난방능력:　5.0kw"]
[null,15,"천정형냉난방","■전원:220/60V"]
[null,null,"15평형 ","■냉방소비전력:　1.8kw"]
[null,null,null,"■난방소비전력:　2.15kw"]
[null,null,null,"■냉방능력:　6.0kw"]
[null,null,null,"■난방능력:　7.2kw"]
[null,16,"천정형냉난방","■전원:220/60V"]
[null,null,"18평형 ","■냉방소비전력:　2.1kw"]
[null,null,null,"■난방소비전력:　2.7kw"]
[null,null,null,"■냉방능력:　7.2kw"]
[null,null,null,"■난방능력:　8.6kw"]
[null,17,"천정형냉난방","■전원:220/60V"]
[null,null,"25평형 ","■냉방소비전력:　2.6kw"]
[null,null,null,"■난방소비전력:　3.2kw"]
[null,null,null,"■냉방능력:　9.0kw"]
[null,null,null,"■난방능력:　11.0kw"]
[null,18,"천정형냉난방","■전원:220/60V"]
[null,null,"28평형 ","■냉방소비전력:　2.8kw"]
[null,null,null,"■난방소비전력:　3.95kw"]
[null,null,null,"■냉방능력:　10.0kw"]
[null,null,null,"■난방능력:　12.9kw"]
[null,19,"천정형냉난방","■전원:220/60V"]
[null,null,"30평형 ","■냉방소비전력:　3.4kw"]
[null,null,null,"■난방소비전력:　4.05kw"]
[null,null,null,"■냉방능력:　11.0kw"]
[null,null,null,"■난방능력:　13.2kw"]
[null,20,"천정형냉난방","■전원:380/60V"]
[null,null,"36평형 ","■냉방소비전력:　4.3kw"]
[null,null,null,"■난방소비전력:　4.8kw"]
[null,null,null,"■냉방능력:　13.0kw"]
[null,null,null,"■난방능력:　15.0kw"]
[null,21,"천정형냉난방","■전원:380/60V"]
[null,null,"40평형 ","■냉방소비전력:　5.1kw"]
[null,null,null,"■난방소비전력:　5.2kw"]
[null,null,null,"■냉방능력:　14.5kw"]
[null,null,null,"■난방능력:　16.7kw"]
[null,22,"천정형냉방","■전원:220/60V"]
[null,null,"10평형 ","■냉방소비전력:　1.12kw"]
[null,null,null,"■냉방능력:　4.0kw"]
[null,23,"천정형냉방","■전원:220/60V"]
[null,null,"15평형 ","■냉방소비전력:　1.78kw"]
[null,null,null,"■냉방능력:　6kw"]
[null,24,"천정형냉방","■전원:220/60V"]
[null,null,"18평형 ","■냉방소비전력:　1.95kw"]
[null,null,null,"■냉방능력:　7.2kw"]
[null,25,"천정형냉방","■전원:220/60V"]
[null,null,"25평형 ","■냉방소비전력:　2.5kw"]
[null,null,null,"■냉방능력:　9.0kw"]
[null,26,"천정형냉방","■전원:220/60V"]
[null,null,"28평형 ","■냉방소비전력:　3.0kw"]
[null,null,null,"■냉방능력:　10.0kw"]
[null,27,"천정형냉방","■전원:220/60V"]
[null,null,"36평형 ","■냉방소비전력:　4.0kw"]
[null,null,null,"■냉방능력:　13.0kw"]
[null,28,"멀티브이실내기 천장형1Way ","■전원:220/60V"]
[null,null,"6평형 ","■냉방소비전력:　0.02kw"]
[null,null,null,"■난방소비전력:　0.02kw"]
[null,null,null,"■냉방능력:　2.3kw"]
[null,null,null,"■난방능력:　2.8kw"]
[null,29,"멀티브이실내기","■전원:220/60V"]
[null,null,"천정형1Way","■냉방소비전력:　0.02kw"]
[null,null,"8평형 ","■난방소비전력:　0.02kw"]
[null,null,null,"■냉방능력:　3.2kw"]
[null,null,null,"■난방능력:　3.6kw"]
[null,30,"멀티브이실내기","■전원:220/60V"]
[null,null,"천정형1Way","■냉방소비전력:　0.03kw"]
[null,null,"10평형 ","■난방소비전력:　0.03kw"]
[null,null,null,"■냉방능력:　4.0kw"]
[null,null,null,"■난방능력:　4.5kw"]
[null,31,"멀티브이실내기","■전원:220/60V"]
[null,null,"천정형4Way","■냉방소비전력:　0.03kw"]
[null,null,"15평형 ","■난방소비전력:　0.03kw"]
[null,null,null,"■냉방능력:　6.0kw"]
[null,null,null,"■난방능력:　6.8kw"]
[null,32,"멀티브이실내기","■전원:220/60V"]
[null,null,"천정형4Way","■냉방소비전력:　0.07kw"]
[null,null,"18평형 ","■난방소비전력:　0.07kw"]
[null,null,null,"■냉방능력:　7.2kw"]
[null,null,null,"■난방능력:　8.1kw"]
[null,33,"멀티브이실내기","■전원:220/60V"]
[null,null,"천정형4Way","■냉방소비전력:　0.07kw"]
[null,null,"23평형 ","■난방소비전력:　0.07kw"]
[null,null,null,"■냉방능력:　8.3kw"]
[null,null,null,"■난방능력:　9.3kw"]
[null,34,"멀티브이실내기","■전원:220/60V"]
[null,null,"천정형4Way","■냉방소비전력:　0.07kw"]
[null,null,"28평형 ","■난방소비전력:　0.07kw"]
[null,null,null,"■냉방능력:　10.0kw"]
[null,null,null,"■난방능력:　11.2kw"]
[null,35,"멀티브이실외기 ","■전원:220/60V"]
[null,null,null,"■냉방소비전력:　3.50kw"]
[null,null,null,"■난방소비전력:　3.58kw"]
[null,null,null,"■냉방능력:　14.5kw"]
[null,null,null,"■난방능력:　16.3kw"]
[null,36,"멀티브이실외기 ","■전원:220/60V"]
[null,null,null,"■냉방소비전력:　4.10kw"]
[null,null,null,"■난방소비전력:　4.10kw"]
[null,null,null,"■냉방능력:　16.0kw"]
[null,null,null,"■난방능력:　18.0kw"]
[null,37,"멀티브이실외기","■전원:380/60V"]
[null,null,null,"■냉방소비전력:　10.0kw"]
[null,null,null,"■난방소비전력:　8.4kw"]
[null,null,null,"■냉방능력:　28.0kw"]
[null,null,null,"■난방능력:　31.5kw"]
[null,38,"멀티브이실외기","■전원:380/60V"]
[null,null,null,"■냉방소비전력:　29.2kw"]
[null,null,null,"■난방소비전력:　32.8kw"]
[null,null,null,"■냉방능력:　2.0kw"]
[null,null,null,"■난방능력:　10.4kw"]
[null,39,"멀티브이실외기","■전원:380/60V"]
[null,null,null,"■냉방소비전력:　2.6kw"]
[null,null,null,"■난방소비전력:　11.6kw"]
[null,null,null,"■냉방능력:　34.8kw"]
[null,null,null,"■난방능력:　39.2kw"]
[null,40,"멀티브이실외기 ","■전원:380/60V"]
[null,null,null,"■냉방소비전력:　2.8kw"]
[null,null,null,"■난방소비전력:　14.5kw"]
[null,null,null,"■냉방능력:　40.6kw"]
[null,null,null,"■난방능력:　45.7kw"]

{"sheet":"시공비","index":1,"n_rows":84,"n_cols":5,"rows_kept":84,"cut":false,"hidden":false,"merged":[[33,3,39,3],[3,2,3,4],[4,3,5,3],[6,3,18,3],[19,3,25,3],[26,3,32,3],[40,3,46,3],[47,3,47,4],[48,3,48,4],[49,3,49,4],[50,2,53,2],[50,3,51,3],[52,3,53,3],[54,3,54,4],[55,2,58,2],[55,3,56,3],[57,3,58,3],[59,2,64,2],[59,3,60,3],[61,3,62,3],[63,3,63,4],[64,3,64,4],[66,3,66,4],[67,2,70,2],[67,3,67,4],[68,3,68,4],[69,3,69,4],[70,3,70,4],[76,3,76,4],[77,2,80,2],[77,3,78,3],[79,3,80,3],[4,2,18,2],[19,2,46,2],[47,2,49,2],[71,2,73,2],[71,3,71,4],[72,3,72,4],[73,3,73,4],[74,2,75,2],[74,3,74,4],[75,3,75,4],[65,2,66,2],[65,3,65,4]]}
[]
[null,null,"<시공비 사양서> - 기기 사양은 별도 탭 참조"]
[]
[null,"순번","구 분"]
[null,1,"인건비\n(잡자재비 포함)","천정형","멀티-카세트형"]
[null,2,null,null,"싱글-카세트형"]
[null,3,null,"기타","10평형"]
[null,4,null,null,"13평형"]
[null,5,null,null,"15평형(PAC)"]
[null,6,null,null,"18평형(PAC)"]
[null,7,null,null,"23평형(PAC)"]
[null,8,null,null,"30평형(PAC)"]
[null,9,null,null,"40평형"]
[null,10,null,null,"58평형"]
[null,11,null,null,"83평형"]
[null,12,null,null,"15평형(인버터)"]
[null,13,null,null,"18평형(인버터)"]
[null,14,null,null,"23평형(인버터)"]
[null,15,null,null,"30평형(인버터)"]
[null,16,"냉매배관(동배관)\n-보온재,전선,통신선\n관부속포함)/\nM당비용","EHP(천정)","RG 38.1 mm"]
[null,17,null,null,"RG 31.8 mm"]
[null,18,null,null,"RG 28.58 mm"]
[null,19,null,null,"RG 25.4 mm"]
[null,20,null,null,"RG 19.05 mm"]
[null,21,null,null,"RG 15.88 mm"]
[null,22,null,null,"RG 12.7 mm"]
[null,23,null,"EHP(벽걸이)","RG 38.1 mm"]
[null,24,null,null,"RG 31.8 mm"]
[null,25,null,null,"RG 28.58 mm"]
[null,26,null,null,"RG 25.4 mm"]
[null,27,null,null,"RG 19.05 mm"]
[null,28,null,null,"RG 15.88 mm"]
[null,29,null,null,"RG 12.7 mm"]
[null,30,null,"EHP(PAC)","RG 38.1 mm"]
[null,31,null,null,"RG 31.8 mm"]
[null,32,null,null,"RG 28.58 mm"]
[null,33,null,null,"RG 25.4 mm"]
[null,34,null,null,"RG 19.05 mm"]
[null,35,null,null,"RG 15.88 mm"]
[null,36,null,null,"RG 12.7 mm"]
[null,37,null,"EHP(인버터)","RG 38.1 mm"]
[null,38,null,null,"RG 31.8 mm"]
[null,39,null,null,"RG 28.58 mm"]
[null,40,null,null,"RG 25.4 mm"]
[null,41,null,null,"RG 19.05 mm"]
[null,42,null,null,"RG 15.88 mm"]
[null,43,null,null,"RG 12.7 mm"]
[null,44,"드레인배관(PVC,VGI,보온재,관부속\n포함)/M당비용","25mm"]
[null,45,null,"32mm"]
[null,46,null,"40mm"]
[null,47,"실외기 앵글제작","천정형 (평형별)","10~23평형"]
[null,48,null,null,"28~40평형"]
[null,49,null,"기타 (평형별)","10~23평형"]
[null,50,null,null,"30~83평형"]
[null,51,"실외기 에어가이드","대당"]
[null,52,"철거작업 (건당)","천정형 (평형별)","10~23평형"]
[null,53,null,null,"28~40평형"]
[null,54,null,"기타 (평형별)","10~23평형"]
[null,55,null,null,"30~83평형"]
[null,56,"이설작업 (건당)","천정형 (평형별)","10~23평형"]
[null,57,null,null,"28~40평형"]
[null,58,null,"기타 (평형별)","10~23평형"]
[null,59,null,null,"30~83평형"]
[null,60,null,"냉매(R22) / kg당"]
[null,61,null,"냉매(R410) / kg당"]
[null,62,"COA 천공","100mm 미만 (구당)"]
[null,63,null,"100mm 이상 (구당)"]
[null,64,"전기공사","단상 (M당)"]
[null,65,null,"삼상 (M당)"]
[null,66,null,"누전차단기 단상 (대당)"]
[null,67,null,"누전차단기 삼상 (대당)"]
[null,68,"배수펌프","8m/h (대당)"]
[null,69,null,"12m/h (대당)"]
[null,70,null,"15m/h (대당)"]
[null,71,"배관마감","외벽 스텐몰딩 (M당)"]
[null,72,null,"내부 스텐몰딩 (M당)"]
[null,73,"실외기패드","콘크리트 (대당)"]
[null,74,"장비반입비","사다리차","반일"]
[null,75,null,null,"전일"]
[null,76,null,"크레인","반일"]
[null,77,null,null,"전일"]
[null,78,"분지관","개당"]
[null,79,"멀티브이실외기받침대","개당"]
[null,80,"싱글형실외기받침대","개당"]